{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["折叠箱配置"],"not_rendered":{"charts":0,"images":18,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"折叠箱配置","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[[20,7,20,10],[29,7,29,10],[32,0,39,0],[23,7,24,10],[40,1,42,2],[1,0,1,10],[29,3,29,4],[5,3,6,3],[32,1,32,3],[40,0,42,0],[28,7,28,10],[36,5,36,10],[4,1,18,1],[26,7,26,10],[38,1,38,3],[28,3,28,4],[30,7,30,10],[39,5,39,10],[19,2,21,2],[3,7,3,10],[33,1,33,3],[23,2,24,2],[19,1,21,1],[4,7,18,10],[21,7,21,10],[19,7,19,10],[40,3,42,10],[27,3,27,4],[38,5,38,10],[27,2,31,2],[31,7,31,10],[37,5,37,10],[2,7,2,10],[27,1,31,1],[39,1,39,3],[3,0,31,0],[31,3,31,4],[36,1,36,3],[35,1,35,3],[35,5,35,10],[25,7,25,10],[0,0,0,10],[34,1,34,3],[33,5,33,10],[34,5,34,10],[4,2,18,2],[30,3,30,4],[37,1,37,3],[27,7,27,10],[23,1,24,1],[32,5,32,10],[22,7,22,10]]}
["折叠式集装箱用材参数及报价单"]
["产品效果图"]
["项目","序号","名称","详细描述","尺寸规格","数量","单位"]
["用\n材\n参\n数","一","型式一\n（Form 1）","标准箱\n(Standard container)","外部尺寸：2500mm（宽）*5800mm（长）*2430m（高）\n内部尺寸：2370mm（宽）*5635mm（长）*2265mm（高） \n折叠尺寸：2500mm（宽）*5800mm（长）*390mm(高）\n重量：1.1t\n40尺高柜：10套",1,"套"]
[null,1,"框架\n(Frame)","顶主梁\n(Top girder)","异形型钢镀锌凹凸管63mm*80mm*1.5mm\nSpecial shaped steel galvanized concave convex pipe 63mm*80mm*1.5mm",2,"组"]
[null,null,null,"底主梁\n(Bottom girder）","镀锌方管50mm*100mm",2,"根"]
[{"$nulls":4},"异形型钢镀锌凹凸管63mm*80mm*1.5mm\nSpecial shaped steel galvanized concave convex pipe 63mm*80mm*1.5mm",2,"组"]
[null,null,null,"顶部横梁\n（Top beam）","镀锌方管50mm*50mm*1.5mm\nGalvanized square pipe 50mm*50mm*1.5mm",3,"根"]
[null,null,null,"顶部次横梁\n（Top sub-beam）","镀锌方管30mm*50mm*1.5mm\nGalvanized square pipe 30mm*50mm*1.5mm",3,"根"]
[null,null,null,"前后端主梁（上侧）\n（Upper side of front and rear main beam）","镀锌方管60mm*60mm*1.5mm\nGalvanized square pipe 60mm*60mm*1.5mm",2,"根"]
[null,null,null,"前后端主梁（下侧）\n（Lower side of front and rear main beam）","异形型钢镀锌凹凸管63mm*80mm*1.5mm\nSpecial shaped steel galvanized concave convex pipe 63mm*80mm*1.5mm",2,"组"]
[null,null,null,"侧墙框架\n（Sidewall frame）","异形型钢镀锌凹凸管63mm*80mm*1.5\nSpecial shaped steel galvanized concave convex pipe 63mm*80mm*1.5",2,"组"]
[null,null,null,"底部横梁\n（Bottom crossbeam）","镀锌方钢管40mm*80mm*1.5mm\nGalvanized square steel pipe 40mm*80mm*1.5mm",9,"根"]
[null,null,null,"前后墙折件立柱\nColumn","镀锌钢管折件 120mm*55mm*2.2mm\nGalvanized steel pipe 120mm*55mm*2.2mm",4,"根"]
[null,null,null,"侧墙中间折件立柱\nSide wall column","镀锌钢u型卡槽折件 150mm*62mm*1.5mm\nGalvanized steel pipe with U-shaped groove 150mm*62mm*1.5mm",2,"组"]
[null,null,null,"顶部吊头\nTop hanging head","钢板180mm*100mm*15mm\nSteel plate（180mm*100mm*15mm）",4,"块"]
[null,null,null,"底部吊头\nBottom hanging head","钢板210mm*100mm*15mm\nSteel plate（210mm*100mm*15mm）",4,"块"]
[null,null,null,"304不锈钢合页\n（304 stainless steel hinge)","高强度镀锌合页85mm*115mm*3mm（轴柱304不锈钢）\nHigh-strength galvanized hinge85mm*115mm*3mm（Shaft column304stainless steel）",36,"个"]
[null,null,null,"整体框架保护涂料\n(Integral frame protective coating）","嘉宝莉高光瓷漆\nCabaret high gloss enamel",1,"套"]
[null,2,"- 屋顶\n（Top of container）","外部顶板\n（External roof）","1040型彩钢瓦（0.45mm）\n1040color steel tile（0.45mm）",6,"张"]
[null,null,null,"内部吊顶\n（Internal ceiling）","831型吊顶瓦（0.28mm）\n831 ceiling tile（0.28mm）",7,"张"]
[null,null,null,"隔热玻璃丝绵\n（Insulation glass wool）","容重60kg/m³厚度30mm\nBulk density 60kg/m³*14.5square",14.5,"㎡"]
[null,3,"- 地面\n（Floor）","玻镁地板（MGO floor）","厚度15mm\n15mm Thickness",5,"张"]
[null,4,"- 墙\n（Wallboard)\n（墙板可定制）","保温隔热岩棉彩钢复合夹芯板（侧墙）\nHeat insulation rock wool color steel composite sandwich panel (side wall)","0.28mm彩钢板/50mm/65kg/m3岩棉\n0.28mm color steel plate / 50mm / 65kg / m3 rock wool",8,"块"]
[null,null,null,"保温隔热岩棉彩钢复合夹芯板（前后墙）\nHeat insulation rock wool color steel composite sandwich panel (Front and rear walls)","0.28mm彩钢板/50mm/65kg/m3岩棉\n0.28mm color steel plate / 50mm / 65kg / m³ rock wool",6,"块"]
[null,5,"-窗\n(Window)","铝合金防盗一体窗推拉系列\naluminum alloy anti-theft integrated window sliding series(push-pull Series)","970mm*1215mm带纱窗\n970mm*1215mm(With screen window)",2,"樘"]
[null,6,"- 门\n(Door)","集装箱专用钢制防盗门\ncontainer special steel anti-theft door","970mm*1970mm",1,"樘"]
[null,7,"- 电气系统\n(Electrical system)","电路保护器\n(circuit protector)",null,1,"个"]
[null,null,null,"标准插座\n（Standard socket）",null,2,"个","（按客户要求的标准）"]
[null,null,null,"单管LED灯 60W\n(Single tube LED light 60W)",null,1,"个"]
[null,null,null,"空调专用插座\n（Special socket for air conditioner）",null,1,"个","（按客户要求的标准）"]
[null,null,null,"灯开关\n(Light switch）",null,1,"个"]
["技\n术\n参\n数","屋面承重",null,null,"≧50公斤/m²"]
[null,"楼面承重",null,null,"≧150公斤/m²"]
[null,"走道承重",null,null,"≧200公斤/m²"]
[null,"壁侧压力",null,null,"≧80公斤/m²"]
[null,"防火级别",null,null,"A级防火"]
[null,"墙变形系数",null,null,"≦300公斤/m²"]
[null,"抗震等级",null,null,"10级抗震"]
[null,"抗风等级",null,null,"10级抗风"]
[null,"备注",null,"安徽泽宇折叠板房和市场上其他折叠板房的区别：\n市场上其他折叠板房折叠处的型材直接采用方管，所有折叠处都要打胶或是加密封条才能起到密封作用，但是打胶是解决不了根本的漏水渗水问题的，几场风雨过后，就会老化，出现缝隙，自然而然的漏水渗水问题就出现了，然后会给使用过程中增添很多麻烦和烦恼。安徽泽宇生产的折叠板房所有折叠处的型材是凹凸卡槽设计，型材自带防水，不用打胶，不管是用到什么时候，永久把风沙雨水，隔离在凹凸卡槽外面，也就是板房体的外面，不会渗进咱们的板房内部。折叠处的合页是304不锈钢轴心合页，他使用的年限也比市场上的其他板房要长，它折叠的次数可以达到在1000次以上！\nThe profiles of other folding board houses on the market are directly used in square tubes. All folding places need to be glued or sealed to play a sealing role. However, gluing cannot solve the fundamental problem of water leakage and seepage. After a few storms, it will age and appear gaps. Naturally, the problem of water leakage and seepage will appear, and then it will add a lot of troubles and troubles to the use process. Anhui Zeyu's production of folding board houses All folding profiles are concave and convex card slot design. The profiles are waterproof and do not need gluing. No matter when they are used, they will permanently isolate the wind, sand and rain from the outside of the concave and convex card slot, that is, the outside of the board house body, and will not penetrate into our board house. The hinge at the folding place is 304 stainless steel axial hinge. His service life is longer than that of other board houses on the market. The number of folds can reach more than 1,000 times!"]