|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Product technical specification** | | | | | | |
| **Product picture** | | **Product dimension drawing** | | | | |
| GS-L1200QG  LED1200W防水切割灯001 | | **YM-4201防水摇头切割灯(1)_23** | | | | |
| **Lamp specification** | | | | | | **parameter** |
| **Product name** | 1400W BSWF IP 4in1 with CMY+CTO | **Product model** | **GS-L1400QG** | | ·Power Supply:AC 100-240V,50/60Hz  ·Power consumption:1800W  ·Light Source:1400W  ·LED life expectancy: 55000 Hours  ·Color Temperature:2700K-6500K  ·Diameter of lens:132mm  ·Color Wheel:linear CMY color mixing,CTO color temperature adjustment (2700K-6500K),  1 color wheel:7 color+white light,Semi- color and rainbow effect;  (adjustable rotating speed and direction)  ·Gobo Wheel:1 static gobo wheel:7 gobos+open;  1 rotating gobo wheel:6 interchangeable gobos+open;  gobo shake(adjustable rotating speed and direction)  ·Animation wheel:Water ripple wheel  ·Prism:6-facet prism,rotatable in both directions  ·Framing shutters: 4x fast and smooth framing shutters, each individually controllable; each blade can block light completely; framing module can be rotated at ±60°  ·Zoom: electronic linear zoom 2°-50°  ·Focus:Variable motorized focus(0-100%)  ·Frost:An independent frost effect  ·Dimmer: 0-100% linear electronic dimmer  ·Strobe: 1-25Hz/s,adjustable speed  ·Movement:Pan: 540°,16 Bit movement resolution  Tilt: 270°,16 Bit movement resolution  Automatically accurate positioning  ·Control mode:DMX512,RDM,Sound,Master/Slave,Auto  ·DMX Channel:22/32/40 CH  ·Protection Rating: IP65  ·Product Size:546\*301\*902mm,N.W.:66.6kg  ·Carton size:720\*470\*1135mm,G.W:75.9kg | |
| **Lamp color** | black | |
| **Net weight** | 66.6kg | **Gross weight** | 75.9kg | |
| **Product size** | 546\*301\*902mm | **Package size** | 720\*470\*1135mm | |
| **Degree of protection** | IP65 | **Lamp material** | Aluminum alloy, high temperature and ultraviolet resistant engineering plastics | |
|  |  |  |  | |
| **Optical system** | | **Effect system** | | |
| **Light source information** | 1400W White LED | **Color wheel** | linear CMY color mixing,CTO color temperature adjustment (2700K-6500K),  1 color wheel:7 color+white light,Semi- color and rainbow effect, (adjustable rotating speed and direction) | |
| **Light source life** | 55000 Hours | **Gobo wheel** | 1 static gobo wheel:7 gobos+open;  1 rotating gobo wheel:6 interchangeable gobos+open;  gobo shake(adjustable rotating speed and direction) | |
| **Color temperature** | 2700K-6500K | **Animation wheel** | Water ripple wheel | |
| **Zoom** | electronic linear zoom 2°-50° | **Prism** | 6-facet prism,rotatable in both directions | |
| **Diameter of lens** | 132mm | **Framing system** | 4x fast and smooth framing shutters, each individually controllable;  each blade can block light completely; framing module can be rotated at ±60° | |
| **Focus** | Variable motorized focus(0-100%) | **Strobe** | 1-25Hz/s,adjustable speed | |
| **Frost** | An independent frost effect | **Dimmer** | 0-100% linear electronic dimmer | |
| **Electrical connection** | | **Control system** | | |
| **Input voltage** | AC 100V-240V, 50/60Hz | **Movement** | Pan: 540°.16 Bit movement resolution; Tilt: 270°,16 Bit movement resolution;  Automatically accurate positioning | |
| **Whole lamp power** | 1800W | **Communication design** | DMX wired / wireless transmission, convenient and fast software upgrade through DMX data cable. | |
| **Signal connection** | 3/5 pin IP65 XLR I / O | **Control Mode** | DMX512,RDM,Sound,Auto,Manual,Master/Slave | |
| **Power connection** | IP66 power head input | **DMX Channel** | 22/32/40 CH | |
| **Display** | LCD digital display,support Chinese & English,Lamps and lanterns can be queried, and the service time of bulbs is convenient for maintenance |  |  | |
| **Other** |  | | | |
| **Gobo+ Color** | | | | **Effect** | | |
| ROTATING GOBO WHEEL :  STATIC GOBO WHEEL :  COLOR WHEEL : | | | | 防水1400W切割灯001防水1400W切割灯002防水1400W切割灯003防水1400W切割灯004 | | |
|  |  |  |  |  |  | |