|  |
| --- |
| Specification |
| \*Product Name | 128 Elements Waterproof Dustproof Cow Fetal Reproductive Disease Wireless USB Ultrasound Scanner Veterinary Ultrasound Machine |
| \*Application scenarios | Engineered for all aspects of bovine and equine reproductive imaging, as well as for equine tendon imaging. |
| \*Elements | 128 |
| \*Imaging Modes | B, M, Color, Power, PW |
| \*Gray scale levels | 256 |
| \*Optional Probes | Rectal linear probe /Rectal convex probe |
| \*Transducer frequency | Rectal linear probe: 6.0-11.0MHzRectal convex probe: 2.0-5.0MHz |
| \*Digital Technology | Tissue harmonic ImagingTissue Specific ImagingPanoramic focusing technologyFrequency compoundingSpace compoundingWide-angle imagingReal-time Dynamic Aperture |
| \*Viewing device | Tablet, Phone, Goggles |
| \*Ultrasound platform | Android, IOS(reserved), Windows(reserved) |
| \*Scanning depth | up to 310mm |
| \*Cine loop | 400 frames movie playback stored |
| \*Waterproof level | IP67 |
| \*Connection Type |  WIFI, USB Type-C |
| \*Product Size | 190x90x60 mm |
| \*Weight | 630g (With probe) |