3颗app超薄电池灯

◆技术参数输入电压：AC100V-250V/50-60HZ

功率：54W

光源： 3颗\*18W高亮度LED灯珠（6合1）

颜色：1670万种颜色变化

防水等级：IP22

光源寿命：50000小时

透镜角度：25° 15° 40°

控制：DMX512、主从控制、自走，2.4G无线DMX512

红外线遥控器控制、 WiFi手机APP控制（支持苹果、安卓系统）

电池：进口18650锂电池4400MAH容量

充电放电可以达到500次以上

充电时间：5小时冲满电

放电时间：RGBWAUV全亮3.5小时、单色15小时，自走模式8小时

通道模式：6CH/8CH/10CH

◆特征

○超薄铝机身散热，

○静音

○数码显示屏（可以显示电量）

○激光打标（可定制图案、LOGO）

○超高频（64KHZ）调光技术、无抖动闪烁

Technical parameters input voltage: ac100v-250v / 50-60Hz

Power: 54W

Light source: 3 \* 18W high brightness LED beads (6 in 1)

Color: 16.7 million color changes

Waterproof grade: IP22

Light source life: 50000 hours

Lens angle: 25° 15 ° 40 °

Control: DMX512, master-slave control, self-propelled, 2.4G wireless DMX512

Infrared remote control WiFi mobile app control (support apple and Android systems)

Battery: imported 18650 lithium battery, 4400mAh capacity

Charging and discharging can reach more than 500 times

Charging time: 5 hours full charge

Discharge time: rgbwauv full bright 3.5 hours, monochrome 15 hours, self-propelled mode 8 hours

Channel mode: 6CH/8CH/10CH

Characteristics

Aluminum body heat dissipation,

The battery can be removed and replaced

\* mute

Digital display screen (can display power)

Laser marking (customizable pattern and logo)

Ultra high frequency (64khz) dimming technology, flicker free