6cs waterproof battery lights

Input voltage: AC100V-250V/50-60HZ

Power: 120W

Light source: 6\* 20W high brightness LED beads (6 in 1)

Shell: All aluminum body, better heat dissipation

Color: 16.7 million color changes

Waterproof grade: IP65

Display: OLED touch screen, convenient and fast, CCT menu key.

Color temperature: 2700-10000K adjustable (300K is a unit)

Time mode: 2 hours/4 hours/6 hours /8hour mode optional

Channel mode:2CH/6CH/8CH/11CH

Light source lifespan: 50000 hours

Lens angle: 10 20

Control: DMX512, master-slave control, self-propelled, 2.4G wireless DMX512

Infrared remote control, WiFi mobile application control (supports Apple and Android)

Battery: Imported 18650 lithium battery with a capacity of 12000MAH

Charging and discharging up to 500 times or more

Charging time: fully charged within 8 hours

Discharge time: RGBWAUV fully lit for 4 hours, monochromatic for 24 hours.

Self mode for 8 hours

◆ Features

○ Self standing suspension

○ Mute

Ultra high frequency (64KHZ) dimming technology with no jitter or flicker

6颗新款防水电池灯

输入电压：AC100V-250V/50-60HZ

功率：120W

光源：6\*20W高亮度LED灯珠（6合1）

外壳：全铝机身，散热更好颜色：1670万次颜色变化

防水等级：IP65

显示：OLED触摸屏，方便快捷，CCT菜单键。

色温：2700-10000K可调（300K为一个单位）

时间模式：2小时/4小时/6小时/8小时模式可选

通道模式：2CH/6CH/8CH/11CH

光源寿命：50000小时

镜头角度：10 20

控制：DMX512，主从控制，自走，2.4G无线DMX512

红外遥控、WiFi手机应用程序控制（支持苹果和Android）

电池：进口18650锂电池12000MAH容量

充放电可达500次以上

充电时间：8小时内充满电

放电时间：RGBWAUV全亮4小时，单色24小时。自走8小时

自行模式8小时

◆ 特征

○ 自立悬挂

○ 静音

○ 超高频（64KHZ）调光技术，无抖动闪烁